**Introduction**

StartBytes\_Transmitter module transmits four zero bytes via SPI to initiate the transmission correctly.

**Signals**

|  |  |  |  |
| --- | --- | --- | --- |
| **Signal** | **Direction** | **Width (bits)** | **Description** |
| CLK | IN | 1 | Not used |
| NRST | IN | 1 | Not used |
| TX\_COUNTER\_MAX | IN | 16 | How many bytes to transmit. Assigned to 4 |
| TX\_COUNTER | OUT | 16 | Not used |
| NEXT\_BYTE | IN | 8 | The next byte to transmit.  Assigned to 0 |